EMpower and Firmware Release Notes

EMpower v2.36.0.3 and receiver Firmware v2.36.0.4 bring various new features and fixes improving flexibility, workflow, and system stability for both CSAMT and A/MT operations.

=======================================
	Operating systems supported
=======================================
	
	Windows
	* Versions tested:
	        Windows 10, 64-bit
	        Windows 11, 64-bit
       Permissions required: Must be logged in as Administrator
	NOTE: Windows 10S and Windows 11S are not supported

	Linux
	* Versions tested:
	        Ubuntu 18.04, 64-bit
	        Ubuntu 20.04.4
	        Permissions required: Standard user
	Mac
	* Versions tested:
	        macOS 10.15.4, Catalina
	        macOS 12.0, Monterey (Apple Silicon)
	        Permissions required: Standard User

=======================================
What's new in the Latest Version
=======================================

Jan 14 2025 : EMpower v2.36.0.3 and Firmware v2.36.0.4

New Features and Fixes:

*PNT plot legend can now be repositioned or hidden.
*Data density (decimation) for white noise recordings is now “long period” by default.
*A warning is now made if saving a config file when Power Recovery is selected but Automatic Start is not.
*EMpower now supports importing of ongoing (partial) recordings, which can be later updated upon reimporting. This is to support ongoing recordings obtained from a data server .
*Can now configure transmitter serial number and type in the prepare section
*Plot title updates with the number of selected sites when multiple processed sites are selected.
*Power recovery function disabled during CSAMT recording.
*Eliminated false error message stating CSAMT electrode contact resistance too low
*Last Selected Tx and TxD saved between sessions
*Time Mask Selection in the Editor renamed “Add Rejection Zone.” 
*Multi-Timeseries Viewer in the Editor renamed “Multi-Instrument Data Viewer.”
*EMpower no longer accepts timeseries of size 0kb
*Recording timeline has improved performance with projects spanning long periods of time.
*OSM Wikimedia Map tiles now download properly.
*Plot axis can now be expanded to the full data range as well as properly zoomed.
*IP address input in the config creator no longer accepts random characters
*Several other minor bug fixes

=====================================
Known Issues for the Latest version:
=====================================

*Low frequency PNT(<100s) may have some issue on full rate recordings
*Mixed use of real and generic receiver calibrations could potentially distort phase curves at high frequencies

***IMPORTANT***
** Please do not open any project in an EMpower version older than 1.54.x.x if the project has already been opened in this version
***IMPORTANT**