DRAFT

EMpower Release Notes

EMpower v2.9.0.11 and receiver Firmware v2.9.0.5 brings Power Recovery for long-term solar-powered installations, along with various new features and fixes improving flexibility, workflow, and system stability for both CSAMT and A/MT operations.

=======================================
	Operating systems supported
=======================================
	
	Windows
	* Versions tested:
	                Windows 10, 64-bit
	                Windows 11, 64-bit
              Permissions required: Must be logged in as Administrator
	NOTE: Windows 10S and Windows 11S are not supported

	Linux
	* Versions tested:
	                Ubuntu 18.04, 64-bit
	                Ubuntu 20.04.4
	                Permissions required: Standard user
	Mac
	* Versions tested:
	                macOS 10.15.4, €Catalina€
	                macOS 12.0, Monterey (Apple Silicon)
	                Permissions required: Standard User

=======================================
What's new in the Latest Version
=======================================

Feb 24 2023 : v2.9.0.11

New Features and Fixes:

*Receivers are now able to power back on automatically when powered by solar battery banks that deplete then become sufficiently charged again
*CSAMT now allows selecting a magnetometer from another receiver
*CSAMT now allows the acquisition schedule to exclude specific frequencies
*Crosspower file now stored in spectral density
*AVGT in EDI files now saves the total number of estimates that are used to calculate each frequency (crosspowers accepted in the editor X crosspowers averaged that make each accepted point in the editor) 
*Added AVGT_SUM in EDI files to save the number of visible accepted crosspowers in the editor
*User will now be alerted if attempting to process data that have a mixture of real and synthetic calibration (including both sensors or receivers)
*Several other minor bug fixes