DRAFT

EMpower Release Notes

EMpower v2.22.0.1 and receiver Firmware v2.22.0.1 brings various new features and fixes improving flexibility, workflow, and system stability for both CSAMT and A/MT operations.

=======================================
	Operating systems supported
=======================================
	
	Windows
	* Versions tested:
	        Windows 10, 64-bit
	        Wndows 11, 64-bit
       Permissions required: Must be logged in as Administrator
	NOTE: Windows 10S and Windows 11S are not supported

	Linux
	* Versions tested:
	        Ubuntu 18.04, 64-bit
	        Ubuntu 20.04.4
	        Permissions required: Standard user
	Mac
	* Versions tested:
	        macOS 10.15.4, €Catalina€
	        macOS 12.0, Monterey (Apple Silicon)
	        Permissions required: Standard User

=======================================
What's new in the Latest Version
=======================================

Mar 28 2024 : v2.22.0.1

New Features and Fixes:

*XX and YY curves of MT data are now processed and displayed 
*Time series viewer now allows display of data from channels of different receivers at the same time
*An existing recording can now be overwritten by a new version with more data when using the network upload feature
*Time series export now includes DC offset data
*Adds support for MTU-5C model “RMT03-L”

*CSAMT stack editor now visually indicates the frequency being edited
*CSAMT and TXD time series data can now be exported to a JSON format
*CSAMT frequency domain field data can now be exported
*Exported CSAMT data now includes the percentage of accepted stacks
*CSAMT prepare window now includes tooltips

*Config creator no longer loses settings changed from the default values before selecting automatic start 
*CSAMT recordings filter now fixed to ensure sites are always visible when selected
*The allowable max and min declination is now +89/-89 in recording information
*Several other minor bug fixes